,Width##LENGTH##INCHES,WaterSense Certified##OTHER##,Waste Water Outlet##OTHER##,Waste Connection##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Vent Connection##OTHER##,Undermount Installation##OTHER##,URL##OTHER##,Type##OTHER##,Pump Electrical Connector##OTHER##,Product Page URL##OTHER##,Product Name##OTHER##,Product Documentation Link##OTHER##,Model##OTHER##,Material##OTHER##,MasterFormat 2014 Name##OTHER##,MasterFormat 2014##OTHER##,Manufacturer Address##OTHER##,Manufacturer##OTHER##,Length##LENGTH##INCHES,Installation Height##LENGTH##INCHES,Hot Water Inlet##OTHER##,Height##LENGTH##INCHES,Heater Electrical Connector##OTHER##,HW Connection##OTHER##,Finish##OTHER##,Environmental Product Declaration##OTHER##,Electrical Note##OTHER##,Electrical Connector##OTHER##,Drop In Installation##OTHER##,Drain Included##OTHER##,Description##OTHER##,Default Elevation##LENGTH##INCHES,Declare Label##OTHER##,Date Modified##OTHER##,Date Created##OTHER##,Copyright##OTHER##,Contact Us##OTHER##,Cold Water Inlet##OTHER##,CW Connection##OTHER##,Blower Electrical Connector##OTHER##,Assembly Code##OTHER##,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,Amplifer Electrical Connector##OTHER##,ADA Compliant##OTHER##
7-Black Black,42.000000000000,0,Waste Water Outlet,1,120.000000000000,0,0,https://www.us.kohler.com/us/,4,Pump Electrical Connector,http://www.us.kohler.com/us/catalog/productDetails.jsp?productId=K-1174-XHGH,Underscore,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-1174-XHGH_spec_US-CA_Kohler_en.pdf,K-1174-XHGH-NY,Acrylic,Residential Bathtubs,22 41 19,"444 Highland Dr.Kohler, WI 53044",Kohler Co.,72.000000000000,0.000000000000,Hot Water Inlet,23.000000000000,Heater Electrical Connector,0,<By Category>,,"Three dedicated circuit required, protected with Class A Ground-Fault Circuit-Interrupter (GFCI) or Residual Current Device (RCD)",1,1,1,"72 Inch x 42 Inch Heated BubbleMassage air bath with whirlpool, center drain",0.000000000000,,02/03/2023,02/22/2019,Copyright Kohler Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,0,Blower Electrical Connector,D2010500,1800.000000000000,Amplifer Electrical Connector,0
58-Thunder Grey,42.000000000000,0,Waste Water Outlet,1,120.000000000000,0,0,https://www.us.kohler.com/us/,6,Pump Electrical Connector,http://www.us.kohler.com/us/catalog/productDetails.jsp?productId=K-1174-XHGH,Underscore,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-1174-XHGH_spec_US-CA_Kohler_en.pdf,K-1174-XHGH-58,Acrylic,Residential Bathtubs,22 41 19,"444 Highland Dr.Kohler, WI 53044",Kohler Co.,72.000000000000,0.000000000000,Hot Water Inlet,23.000000000000,Heater Electrical Connector,0,Kohler-Acrylic-58-Thunder_Grey,,"Three dedicated circuit required, protected with Class A Ground-Fault Circuit-Interrupter (GFCI) or Residual Current Device (RCD)",1,1,1,"72 Inch x 42 Inch Heated BubbleMassage air bath with whirlpool, center drain",0.000000000000,,02/03/2023,02/22/2019,Copyright Kohler Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,0,Blower Electrical Connector,D2010500,1800.000000000000,Amplifer Electrical Connector,0
95-Ice Grey,42.000000000000,0,Waste Water Outlet,1,120.000000000000,0,0,https://www.us.kohler.com/us/,5,Pump Electrical Connector,http://www.us.kohler.com/us/catalog/productDetails.jsp?productId=K-1174-XHGH,Underscore,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-1174-XHGH_spec_US-CA_Kohler_en.pdf,K-1174-XHGH-95,Acrylic,Residential Bathtubs,22 41 19,"444 Highland Dr.Kohler, WI 53044",Kohler Co.,72.000000000000,0.000000000000,Hot Water Inlet,23.000000000000,Heater Electrical Connector,0,Kohler-Acrylic-95-Ice_Grey,,"Three dedicated circuit required, protected with Class A Ground-Fault Circuit-Interrupter (GFCI) or Residual Current Device (RCD)",1,1,1,"72 Inch x 42 Inch Heated BubbleMassage air bath with whirlpool, center drain",0.000000000000,,02/03/2023,02/22/2019,Copyright Kohler Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,0,Blower Electrical Connector,D2010500,1800.000000000000,Amplifer Electrical Connector,0
NY-Dune,42.000000000000,0,Waste Water Outlet,1,120.000000000000,0,0,https://www.us.kohler.com/us/,4,Pump Electrical Connector,http://www.us.kohler.com/us/catalog/productDetails.jsp?productId=K-1174-XHGH,Underscore,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-1174-XHGH_spec_US-CA_Kohler_en.pdf,K-1174-XHGH-NY,Acrylic,Residential Bathtubs,22 41 19,"444 Highland Dr.Kohler, WI 53044",Kohler Co.,72.000000000000,0.000000000000,Hot Water Inlet,23.000000000000,Heater Electrical Connector,0,<By Category>,,"Three dedicated circuit required, protected with Class A Ground-Fault Circuit-Interrupter (GFCI) or Residual Current Device (RCD)",1,1,1,"72 Inch x 42 Inch Heated BubbleMassage air bath with whirlpool, center drain",0.000000000000,,02/03/2023,02/22/2019,Copyright Kohler Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,0,Blower Electrical Connector,D2010500,1800.000000000000,Amplifer Electrical Connector,0
47-Almond,42.000000000000,0,Waste Water Outlet,1,120.000000000000,0,0,https://www.us.kohler.com/us/,3,Pump Electrical Connector,http://www.us.kohler.com/us/catalog/productDetails.jsp?productId=K-1174-XHGH,Underscore,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-1174-XHGH_spec_US-CA_Kohler_en.pdf,K-1174-XHGH-47,Acrylic,Residential Bathtubs,22 41 19,"444 Highland Dr.Kohler, WI 53044",Kohler Co.,72.000000000000,0.000000000000,Hot Water Inlet,23.000000000000,Heater Electrical Connector,0,Kohler-Acrylic-47-Almond,,"Three dedicated circuit required, protected with Class A Ground-Fault Circuit-Interrupter (GFCI) or Residual Current Device (RCD)",1,1,1,"72 Inch x 42 Inch Heated BubbleMassage air bath with whirlpool, center drain",0.000000000000,,02/03/2023,02/22/2019,Copyright Kohler Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,0,Blower Electrical Connector,D2010500,1800.000000000000,Amplifer Electrical Connector,0
96-Biscuit,42.000000000000,0,Waste Water Outlet,1,120.000000000000,0,0,https://www.us.kohler.com/us/,2,Pump Electrical Connector,http://www.us.kohler.com/us/catalog/productDetails.jsp?productId=K-1174-XHGH,Underscore,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-1174-XHGH_spec_US-CA_Kohler_en.pdf,K-1174-XHGH-96,Acrylic,Residential Bathtubs,22 41 19,"444 Highland Dr.Kohler, WI 53044",Kohler Co.,72.000000000000,0.000000000000,Hot Water Inlet,23.000000000000,Heater Electrical Connector,0,Kohler-Acrylic-96-Biscuit,,"Three dedicated circuit required, protected with Class A Ground-Fault Circuit-Interrupter (GFCI) or Residual Current Device (RCD)",1,1,1,"72 Inch x 42 Inch Heated BubbleMassage air bath with whirlpool, center drain",0.000000000000,,02/03/2023,02/22/2019,Copyright Kohler Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,0,Blower Electrical Connector,D2010500,1800.000000000000,Amplifer Electrical Connector,0
0-White,42.000000000000,0,Waste Water Outlet,1,120.000000000000,0,0,https://www.us.kohler.com/us/,1,Pump Electrical Connector,http://www.us.kohler.com/us/catalog/productDetails.jsp?productId=K-1174-XHGH,Underscore,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-1174-XHGH_spec_US-CA_Kohler_en.pdf,K-1174-XHGH-0,Acrylic,Residential Bathtubs,22 41 19,"444 Highland Dr.Kohler, WI 53044",Kohler Co.,72.000000000000,0.000000000000,Hot Water Inlet,23.000000000000,Heater Electrical Connector,0,Kohler-Acrylic-0-White,,"Three dedicated circuit required, protected with Class A Ground-Fault Circuit-Interrupter (GFCI) or Residual Current Device (RCD)",1,1,1,"72 Inch x 42 Inch Heated BubbleMassage air bath with whirlpool, center drain",0.000000000000,,02/03/2023,02/22/2019,Copyright Kohler Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,0,Blower Electrical Connector,D2010500,1800.000000000000,Amplifer Electrical Connector,0
