,Width##LENGTH##INCHES,WaterSense Certified##OTHER##,Waste Water Outlet##OTHER##,Waste Connection##OTHER##,Vent Connection##OTHER##,URL##OTHER##,Type##OTHER##,Toilet Length##LENGTH##INCHES,Secondary Finish##OTHER##,Seconadry Material##OTHER##,Seat Included##OTHER##,Rough-In##LENGTH##INCHES,Product Page URL##OTHER##,Product Name##OTHER##,Product Documentation Link##OTHER##,Pressure##PIPING_PRESSURE##POUNDS_FORCE_PER_SQUARE_INCH,Model##OTHER##,Material##OTHER##,Master Format 2014 Name##OTHER##,Master Format 2014##OTHER##,Manufacturer Address##OTHER##,Manufacturer##OTHER##,Length##LENGTH##INCHES,Hot Water Inlet##OTHER##,Height##LENGTH##INCHES,HW Connection##OTHER##,Flush Rate- LPF##OTHER##,Flush Rate- GPF##OTHER##,Flow Rate##PIPING_FLOW##US_GALLONS_PER_MINUTE,Finish##OTHER##,Environmental Product Declaration##OTHER##,Description##OTHER##,Default Elevation##LENGTH##INCHES,Declare Label##OTHER##,Date Modified##OTHER##,Date Created##OTHER##,Copyright##OTHER##,Contact Us##OTHER##,Cold Water Inlet##OTHER##,CW Connection##OTHER##,Bowl Height##LENGTH##INCHES,Assembly Code##OTHER##,ADA Compliant##OTHER##
"1.28 GPF, DC Powered",14.566406250000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,1,26.378906250000,Kohler-Metal-CP-Polished_Chrome,Brass Construction,0,12.014960629921,http://www.us.kohler.com/us/catalog/productDetails.jsp?productNumber=PR96057-T4D,Highcliff Ultra,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR96057-T4D_spec_US-CA_Kohler_en.pdf,79.999996598362,K-PR96057-T4D-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",Kohler Co.,30.000000000000,Hot Water Inlet,33.503906250000,0,4.86 LPF,1.28 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-96057.pdf,Commercial toilet with Mach Tripoint touchless DC 1.28 gpf flushometer,0.000000000000,,09/15/2025,11/24/2021,Copyright Kohler Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,16.613281250000,D2010100,1
"1.28 GPF, Hybrid Powered",14.566406250000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,2,26.378906250000,Kohler-Metal-CP-Polished_Chrome,Brass Construction,0,12.014960629921,http://www.us.kohler.com/us/catalog/productDetails.jsp?productNumber=PR96057-T4H,Highcliff Ultra,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR96057-T4H_spec_US-CA_Kohler_en.pdf,79.999996598362,K-PR96057-T4H-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",Kohler Co.,30.000000000000,Hot Water Inlet,33.503906250000,0,4.86 LPF,1.28 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-96057.pdf,Commercial toilet with Mach Tripoint touchless 1.28 gpf HES-powered flushometer,0.000000000000,,09/15/2025,11/24/2021,Copyright Kohler Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,16.613281250000,D2010100,1
"1.0 GPF, DC Powered",14.566406250000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,3,26.378906250000,Kohler-Metal-CP-Polished_Chrome,Brass Construction,0,12.014960629921,http://www.us.kohler.com/us/catalog/productDetails.jsp?productNumber=PR96057-T3D,Highcliff Ultra,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR96057-T3D_spec_US-CA_Kohler_en.pdf,79.999996598362,K-PR96057-T3D-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",Kohler Co.,30.000000000000,Hot Water Inlet,33.503906250000,0,3.8 LPF,1.0 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-96057.pdf,Commercial toilet with Mach Tripoint touchless DC 1.0 gpf flushometer,0.000000000000,,09/15/2025,11/24/2021,Copyright Kohler Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,16.613281250000,D2010100,1
"1.0 GPF, Hybrid Powered",14.566406250000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,4,26.378906250000,Kohler-Metal-CP-Polished_Chrome,Brass Construction,0,12.014960629921,http://www.us.kohler.com/us/catalog/productDetails.jsp?productNumber=PR96057-T3H,Highcliff Ultra,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR96057-T3H_spec_US-CA_Kohler_en.pdf,79.999996598362,K-PR96057-T3H-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",Kohler Co.,30.000000000000,Hot Water Inlet,33.503906250000,0,3.8 LPF,1.0 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-96057.pdf,Commercial toilet with Mach Tripoint touchless 1.0 gpf HES-powered flushometer,0.000000000000,,09/15/2025,11/24/2021,Copyright Kohler Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,16.613281250000,D2010100,1
"1.6 GPF, DC Powered",14.566406250000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,5,26.378906250000,Kohler-Metal-CP-Polished_Chrome,Brass Construction,0,12.014960629921,http://www.us.kohler.com/us/catalog/productDetails.jsp?productNumber=PR96057-T5D,Highcliff Ultra,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR96057-T5D_spec_US-CA_Kohler_en.pdf,79.999996598362,K-PR96057-T5D-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",Kohler Co.,30.000000000000,Hot Water Inlet,33.503906250000,0,6.08 LPF,1.6 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-96057.pdf,Commercial toilet with Mach Tripoint touchless DC 1.6 gpf flushometer,0.000000000000,,09/15/2025,11/24/2021,Copyright Kohler Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,16.613281250000,D2010100,1
"1.28 GPF, DC Powered, Antimicrobial",14.566406250000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,6,26.378906250000,Kohler-Metal-CP-Polished_Chrome,Brass Construction,0,12.014960629921,http://www.us.kohler.com/us/catalog/productDetails.jsp?productNumber=PR96057-T4DS,Highcliff Ultra,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR96057-T4DS_spec_US-CA_Kohler_en.pdf,79.999996598362,K-PR96057-T4DS-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",Kohler Co.,30.000000000000,Hot Water Inlet,33.503906250000,0,4.86 LPF,1.28 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-96057.pdf,Antimicrobial toilet with Mach Tripoint touchless DC 1.28 gpf flushometer,0.000000000000,,09/15/2025,11/24/2021,Copyright Kohler Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,16.613281250000,D2010100,1
"1.28 GPF, Hybrid Powered, Antimicrobial",14.566406250000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,7,26.378906250000,Kohler-Metal-CP-Polished_Chrome,Brass Construction,0,12.014960629921,http://www.us.kohler.com/us/catalog/productDetails.jsp?productNumber=PR96057-T4HS,Highcliff Ultra,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR96057-T4HS_spec_US-CA_Kohler_en.pdf,79.999996598362,K-PR96057-T4HS-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",Kohler Co.,30.000000000000,Hot Water Inlet,33.503906250000,0,4.86 LPF,1.28 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-96057.pdf,Antimicrobial toilet with Mach Tripoint touchless 1.28 gpf HES-powered flushometer,0.000000000000,,09/15/2025,11/24/2021,Copyright Kohler Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,16.613281250000,D2010100,1
"1.0 GPF, DC Powered, Antimicrobial",14.566406250000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,8,26.378906250000,Kohler-Metal-CP-Polished_Chrome,Brass Construction,0,12.014960629921,http://www.us.kohler.com/us/catalog/productDetails.jsp?productNumber=PR96057-T3DS,Highcliff Ultra,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR96057-T3DS_spec_US-CA_Kohler_en.pdf,79.999996598362,K-PR96057-T3DS-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",Kohler Co.,30.000000000000,Hot Water Inlet,33.503906250000,0,3.8 LPF,1.0 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-96057.pdf,Antimicrobial toilet with Mach Tripoint touchless DC 1.0 gpf flushometer,0.000000000000,,09/15/2025,11/24/2021,Copyright Kohler Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,16.613281250000,D2010100,1
"1.0 GPF, Hybrid Powered, Antimicrobial",14.566406250000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,9,26.378906250000,Kohler-Metal-CP-Polished_Chrome,Brass Construction,0,12.014960629921,http://www.us.kohler.com/us/catalog/productDetails.jsp?productNumber=PR96057-T3HS,Highcliff Ultra,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR96057-T3HS_spec_US-CA_Kohler_en.pdf,79.999996598362,K-PR96057-T3HS-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",Kohler Co.,30.000000000000,Hot Water Inlet,33.503906250000,0,3.8 LPF,1.0 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-96057.pdf,Antimicrobial toilet with Mach Tripoint touchless 1.0 gpf HES-powered flushometer,0.000000000000,,09/15/2025,11/24/2021,Copyright Kohler Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,16.613281250000,D2010100,1
"1.6 GPF, DC Powered, Antimicrobial",14.566406250000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,10,26.378906250000,Kohler-Metal-CP-Polished_Chrome,Brass Construction,0,12.014960629921,http://www.us.kohler.com/us/catalog/productDetails.jsp?productNumber=PR96057-T5DS,Highcliff Ultra,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR96057-T5DS_spec_US-CA_Kohler_en.pdf,79.999996598362,K-PR96057-T5DS-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",Kohler Co.,30.000000000000,Hot Water Inlet,33.503906250000,0,6.08 LPF,1.6 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-96057.pdf,Antimicrobial toilet with Mach Tripoint touchless DC 1.6 gpf flushometer,0.000000000000,,09/15/2025,11/24/2021,Copyright Kohler Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,16.613281250000,D2010100,1
