,Width##LENGTH##INCHES,WaterSense Certified##OTHER##,Waste Water Outlet##OTHER##,Waste Connection##OTHER##,Vent Connection##OTHER##,URL##OTHER##,Type##OTHER##,Secondary Finish##OTHER##,Seat Included##OTHER##,Rough-In##LENGTH##INCHES,Product Page URL##OTHER##,Product Name##OTHER##,Product Documentation Link##OTHER##,Pressure##PIPING_PRESSURE##POUNDS_FORCE_PER_SQUARE_INCH,Model##OTHER##,Material##OTHER##,Master Format 2014 Name##OTHER##,Master Format 2014##OTHER##,Manufacturer Address##OTHER##,Manufacturer##OTHER##,Length##LENGTH##INCHES,Hot Water Inlet##OTHER##,Height##LENGTH##INCHES,HW Connection##OTHER##,Flush Rate- LPF##OTHER##,Flush Rate- GPF##OTHER##,Flow Rate##PIPING_FLOW##GALLONS_US_PER_MINUTE,Finish##OTHER##,Environmental Product Declaration##OTHER##,Description##OTHER##,Default Elevation##LENGTH##INCHES,Declare Label##OTHER##,Date Modified##OTHER##,Date Created##OTHER##,Copyright##OTHER##,Contact Us##OTHER##,Cold Water Inlet##OTHER##,CW Connection##OTHER##,Bedpan Lugs##OTHER##,Assembly Code##OTHER##,ADA Compliant##OTHER##
"1.28 GPF, DC Powered, Antimicrobial",16.781250000000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,1,Kohler-Metal-CP-Polished_Chrome,0,5.000000000000,http://www.us.kohler.com/us/catalog/productDetails.jsp?productId=PR25042-T4DS,Modflex_Adjust-a-Bowl,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR25042-T4DS_spec_US-CA_Kohler_en.pdf,80.000000000000,K-PR25042-T4DS-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",KOHLER Co.,26.867187500000,Hot Water Inlet,34.265625000000,0,4.84 LPF,1.28 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-25042.pdf,MODFLEX BOWL & MACH 1.28 GPF DC COMBO,0.000000000000,,11/24/2021,11/24/2021,Copyright KOHLER Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,0,D2010100,1
"1.28 GPF, Hybrid Powered, Antimicrobial",16.781250000000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,2,Kohler-Metal-CP-Polished_Chrome,0,5.000000000000,http://www.us.kohler.com/us/catalog/productDetails.jsp?productId=PR25042-T4HS,Modflex_Adjust-a-Bowl,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR25042-T4HS_spec_US-CA_Kohler_en.pdf,80.000000000000,K-PR25042-T4HS-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",KOHLER Co.,26.867187500000,Hot Water Inlet,34.265625000000,0,4.84 LPF,1.28 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-25042.pdf,MODFLEX BOWL & MACH 1.28 GPF HYBRID COMBO,0.000000000000,,11/24/2021,11/24/2021,Copyright KOHLER Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,0,D2010100,1
"1.0 GPF, DC Powered, Antimicrobial",16.781250000000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,3,Kohler-Metal-CP-Polished_Chrome,0,5.000000000000,http://www.us.kohler.com/us/catalog/productDetails.jsp?productId=PR25042-T3DS,Modflex_Adjust-a-Bowl,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR25042-T3DS_spec_US-CA_Kohler_en.pdf,80.000000000000,K-PR25042-T3DS-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",KOHLER Co.,26.867187500000,Hot Water Inlet,34.265625000000,0,3.78 LPF,1.0 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-25042.pdf,MODFLEX BOWL & MACH 1.0 GPF DC COMBO,0.000000000000,,11/24/2021,11/24/2021,Copyright KOHLER Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,0,D2010100,1
"1.0 GPF, Hybrid Powered, Antimicrobial",16.781250000000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,4,Kohler-Metal-CP-Polished_Chrome,0,5.000000000000,http://www.us.kohler.com/us/catalog/productDetails.jsp?productId=PR25042-T3HS,Modflex_Adjust-a-Bowl,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR25042-T3HS_spec_US-CA_Kohler_en.pdf,80.000000000000,K-PR25042-T3HS-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",KOHLER Co.,26.867187500000,Hot Water Inlet,34.265625000000,0,3.78 LPF,1.0 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-25042.pdf,MODFLEX BOWL & MACH 1.0 GPF HYBRID COMBO,0.000000000000,,11/24/2021,11/24/2021,Copyright KOHLER Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,0,D2010100,1
"1.6 GPF, DC Powered, Antimicrobial",16.781250000000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,5,Kohler-Metal-CP-Polished_Chrome,0,5.000000000000,http://www.us.kohler.com/us/catalog/productDetails.jsp?productId=PR25042-T5DS,Modflex_Adjust-a-Bowl,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR25042-T5DS_spec_US-CA_Kohler_en.pdf,80.000000000000,K-PR25042-T5DS-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",KOHLER Co.,26.867187500000,Hot Water Inlet,34.265625000000,0,6.05 LPF,1.6 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-25042.pdf,MODFLEX BOWL & MACH 1.6 GPF DC COMBO,0.000000000000,,11/24/2021,11/24/2021,Copyright KOHLER Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,0,D2010100,1
"1.28 GPF, DC Powered, Antimicrobial, Bedpan Lugs",16.781250000000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,6,Kohler-Metal-CP-Polished_Chrome,0,5.000000000000,http://www.us.kohler.com/us/catalog/productDetails.jsp?productId=PR25042-T4DSL,Modflex_Adjust-a-Bowl,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR25042-T4DSL_spec_US-CA_Kohler_en.pdf,80.000000000000,K-PR25042-T4DSL-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",KOHLER Co.,26.867187500000,Hot Water Inlet,34.265625000000,0,4.84 LPF,1.28 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-25042.pdf,MODFLEX BOWL WITH BEDPANLUGS & MACH 1.28 GPF DC COMBO,0.000000000000,,11/24/2021,11/24/2021,Copyright KOHLER Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,1,D2010100,1
"1.28 GPF, Hybrid Powered, Antimicrobial, Bedpan Lugs",16.781250000000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,7,Kohler-Metal-CP-Polished_Chrome,0,5.000000000000,http://www.us.kohler.com/us/catalog/productDetails.jsp?productId=PR25042-T4HSL,Modflex_Adjust-a-Bowl,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR25042-T4HSL_spec_US-CA_Kohler_en.pdf,80.000000000000,K-PR25042-T4HSL-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",KOHLER Co.,26.867187500000,Hot Water Inlet,34.265625000000,0,4.84 LPF,1.28 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-25042.pdf,MODFLEX BOWL WITH BEDPANLUGS & MACH 1.28 GPF HYBRID COMBO,0.000000000000,,11/24/2021,11/24/2021,Copyright KOHLER Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,1,D2010100,1
"1.0 GPF, DC Powered, Antimicrobial, Bedpan Lugs",16.781250000000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,8,Kohler-Metal-CP-Polished_Chrome,0,5.000000000000,http://www.us.kohler.com/us/catalog/productDetails.jsp?productId=PR25042-T3DSL,Modflex_Adjust-a-Bowl,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR25042-T3DSL_spec_US-CA_Kohler_en.pdf,80.000000000000,K-PR25042-T3DSL-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",KOHLER Co.,26.867187500000,Hot Water Inlet,34.265625000000,0,3.78 LPF,1.0 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-25042.pdf,MODFLEX BOWL WITH BEDPANLUGS & MACH 1.0 GPF DC COMBO,0.000000000000,,11/24/2021,11/24/2021,Copyright KOHLER Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,1,D2010100,1
"1.0 GPF, Hybrid Powered, Antimicrobial, Bedpan Lugs",16.781250000000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,9,Kohler-Metal-CP-Polished_Chrome,0,5.000000000000,http://www.us.kohler.com/us/catalog/productDetails.jsp?productId=PR25042-T3HSL,Modflex_Adjust-a-Bowl,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR25042-T3HSL_spec_US-CA_Kohler_en.pdf,80.000000000000,K-PR25042-T3HSL-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",KOHLER Co.,26.867187500000,Hot Water Inlet,34.265625000000,0,3.78 LPF,1.0 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-25042.pdf,MODFLEX WITH BEDPANLUGS & MACH 1.0 GPF HYBRID COMBO,0.000000000000,,11/24/2021,11/24/2021,Copyright KOHLER Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,1,D2010100,1
"1.6 GPF, DC Powered, Antimicrobial, Bedpan Lugs",16.781250000000,1,Waste Water Outlet,1,0,https://www.us.kohler.com/us/,10,Kohler-Metal-CP-Polished_Chrome,0,5.000000000000,http://www.us.kohler.com/us/catalog/productDetails.jsp?productId=PR25042-T5DSL,Modflex_Adjust-a-Bowl,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-PR25042-T5DSL_spec_US-CA_Kohler_en.pdf,80.000000000000,K-PR25042-T5DSL-NA,Vitreous China,Residential Water Closets,22 42 13.13,"444 Highland Dr, Kohler, WI 53044",KOHLER Co.,26.867187500000,Hot Water Inlet,34.265625000000,0,6.05 LPF,1.6 GPF,25.000000000000,Kohler-Vitreous_China-0-White,https://www.us.kohler.com/webassets/kpna/catalog/pdf/en/K-25042.pdf,MODFLEX BOWL WITH BEDPANLUGS & MACH 1.6 GPF DC COMBO,0.000000000000,,11/24/2021,11/24/2021,Copyright KOHLER Co.,https://www.us.kohler.com/us/static/contact.jsp,Cold Water Inlet,1,1,D2010100,1
